{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","","","30","34"]
["","","Soojendamine","Ülimadal","m³/min","","","32","34"]
["Helivõimsustase","Soojendamine","","","dBA","","62","","","62"]
["","Jahutamine","","","dBA","","60","","","60"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","cfm","","","1059","1200"]
["","","Soojendamine","Ülimadal","cfm","","","1130","1200"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550","550","550","550","550"]
["","","","Laius","mm","765","765","765","765","765","765"]
["","","","Sügavus","mm","285","285","285","285","285","285"]
["Kaal","Ühik","","","kg","36","36","36","41","41","41"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","500","500","760","890","500","500"]
["","","Soojendamine","Ülimadal","p/min","320","320","820","890","500","500"]
["Compressor","Type","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","","46.0","-10","-10","46.0"]
["","","","Max","°CDB","","-10","46","46","-10"]
["","Küte","Keskkond","Min","°CWB","","-15","-15","-15","-15.0"]
["","","","Max","°CWB","","18.0","18","18","18.0"]
["Mürarõhutase","Jahutus","","kiire","dBA","46","46","","","48","48"]
["","","","Nom","dBA","","","48","46"]
["","Küte","","kiire","dBA","48","48","","","50","50"]
["","","","Nom","dBA","","","50","48"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Kogus","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Kogus","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)","002 (torustikule mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Max","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","30","30","30","30","30","30"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","50"]
["","Pinge","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Märkused","","","","","(1) - Ühe ruumi jaoks","","(1) - Sisaldav fluoritud kasvuhoonegaase","","","(1) - Ühe ruumi jaoks"]
["","","","","","","(1) - Ühe ruumi jaoks","","","(1) - Ühe ruumi jaoks"]
["","","","","","","(2) - Vt töövahemiku kohta eraldi joonist","","","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","(3) - Vt eraldi elektriandmete joonist","","","(3) - Vt eraldi elektriandmete joonist"]
["","","","","","","(4) - Sisaldav fluoritud kasvuhoonegaase","","","(4) - Sisaldav fluoritud kasvuhoonegaase"]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor"]
["Standardsed lisatarvikud","Reducer assembly","","","","","","","1","1","1"]