{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Mõõtmed","Ühik","","Kõrgus","mm","552","734"]
["","","","Laius","mm","852","974"]
["","","","Sügavus","mm","350","408"]
["Kaal","Ühik","","","kg","41","60"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-10","-10"]
["","","","Max","° CDB","50","50"]
["Mürarõhutase","Jahutus","","Nom","dBA","48","48"]
["","Küte","","Nom","dBA","50","48"]
["Külmaaine","Tüüp","","","","R-32","R-32"]
["","Kogus","","","kg","1.15","2.00"]
["","Kogus","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20 (1)","25 (1)"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15","15"]
["","","IU - IU","Max","m","7.5","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","30","50"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Drain cap","","","","","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Märkused","","","","","(1) - Ühe ruumi jaoks","(1) - Ühe ruumi jaoks"]
["","","","","","(2) - Mudelitega CVXM-A, FVXM-A kombineerimisel – maksimaalne torustiku pikkus on 30m.","(2) - Mudelitega CVXM-A, FVXM-A kombineerimisel – maksimaalne torustiku pikkus on 30m."]
["","","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]
["","","","","","(5) - Sisaldav fluoritud kasvuhoonegaase","(5) - Sisaldav fluoritud kasvuhoonegaase"]