{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Mürarõhutase","Küte","","Nom","dBA","48","48","","50","50"]
["","Jahutus","","Nom","dBA","47","47","","48","48"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1","","1","1"]
["","Kruvide kott","","","","1","1","","1","1"]
["","Tühjendusava kork","","","","1","1","","1","1"]
["Jahutusaine","Charge","","","tCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Täide","","","kg","1.20","1.20","","1.60","1.60"]
["","Tüüp","","","","R-410A","R-410A","","R-410A","R-410A"]
["Torustikuühendused","Kõrguste vahe","IU - IU","Max","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max","m","15","15","","15","15"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)","","0,02 (torustikule, mille pikkus ületab 20 m)","0,02 (torustikule, mille pikkus ületab 20 m)"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","30","30","","30","30"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","765","765","","765","765"]
["","","","Sügavus","mm","285","285","","285","285"]
["","","","Kõrgus","mm","550","550","","550","550"]
["Kaal","Ühik","","","kg","38","38","","42","42"]
["Power supply","Faas","","","","1~","1~","","1~","1~"]
["","Sagedus","","","Hz","50","50","","50","50"]
["","Pinge","","","V","220-240","220-240","","220-240","220-240"]
["Märkused","","","","","(1) - Sisaldav fluoritud kasvuhoonegaase","(1) - Sisaldav fluoritud kasvuhoonegaase","","(1) - Sisaldav fluoritud kasvuhoonegaase","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","550","","","550"]
["","","","Laius","mm","","","765","","","765"]
["","","","Sügavus","mm","","","285","","","285"]
["Kaal","Ühik","","","kg","","","38","","","42"]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","","","10","","","10"]
["","","","Max","° CDB","","","46","","","46"]
["","Küte","Keskkond","Min","°CWB","","","-15","","","-15"]
["","","","Max","°CWB","","","15.5","","","15.5"]
["Mürarõhutase","Jahutus","","Nom","dBA","","","47","","","48"]
["","Küte","","Nom","dBA","","","48","","","50"]
["Külmaaine","Tüüp","","","","","","R-410A","","","R-410A"]
["","Kogus","","","kg","","","1.20","","","1.60"]
["","Kogus","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","","20","","","20"]
["","Jahutusaine lisatäide","","","kg/m","","","0,02 (torustikule, mille pikkus ületab 20 m)","","","0,02 (torustikule, mille pikkus ületab 20 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","","15","","","15"]
["","","IU - IU","Max","m","","","7.5","","","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","","","30","","","30"]
["Standardsed lisatarvikud","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Elektritoide","Faas","","","","","","1~","","","1~"]
["","Sagedus","","","Hz","","","50","","","50"]
["","Pinge","","","V","","","220-240","","","220-240"]
["Standardsed lisatarvikud","Siirdmikusõlm","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]