{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Mürarõhutase","Küte","","Nom","dBA","47"]
["","Jahutus","","Nom","dBA","46"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kruvide kott","","","","1"]
["","Tühjendusava kork","","","","1"]
["","Äravoolukork (1)","","","","6"]
["","Äravoolukork (2)","","","","3"]
["","Mahakooritav F-gaasi märgis","","","","1"]
["","Täiendav jahutusaine kleebis","","","","1"]
["Jahutusaine","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Tüüp","","","","R-32"]
["Ventilaatori mootor","Kiirus","Jahutus","Ülimadal","p/min","420"]
["","","Küte","Ülimadal","p/min","420"]
["Torustikuühendused","Kõrguste vahe","IU - IU","Max","m","7.5"]
["","","IU - OU","Max","m","15"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","50"]
["Compressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","868"]
["","","","Sügavus","mm","320"]
["","","","Kõrgus","mm","734"]
["Kaal","Ühik","","","kg","57"]
["Power supply","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(3) - Vt eraldi elektriandmete joonist"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","","24"]
["","","Soojendamine","Ülimadal","m³/min","","24"]
["","","","Ülimadal","cfm","","847"]
["","","Soojendamine","Ülimadal","cfm","","847"]
["Mõõtmed","Ühik","","Kõrgus","mm","","734"]
["","","","Laius","mm","","868"]
["","","","Sügavus","mm","","320"]
["Kaal","Ühik","","","kg","","57"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","","420"]
["","","Soojendamine","Ülimadal","p/min","","420"]
["Compressor","Tüüp","","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","","-10"]
["","","","Max","° CDB","","46"]
["","Küte","Keskkond","Min","°CWB","","-15"]
["","","","Max","°CWB","","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","","46"]
["","Küte","","Nom","dBA","","47"]
["Külmaaine","Tüüp","","","","","R-32"]
["","Kogus","","","kg","","1.80"]
["","Kogus","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","25"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","15"]
["","","IU - IU","Max","m","","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","","50"]
["Standardsed lisatarvikud","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Elektritoide","Faas","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]