{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","","","24.1"]
["","","Soojendamine","Ülimadal","m³/min","","","24.1"]
["","","","Ülimadal","cfm","","","851"]
["","","Soojendamine","Ülimadal","cfm","","","851"]
["Mõõtmed","Ühik","","Kõrgus","mm","734","734","734"]
["","","","Laius","mm","974","974","958"]
["","","","Sügavus","mm","401","401","340"]
["Kaal","Ühik","","","kg","57","57","62"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","420","420"]
["","","Soojendamine","Ülimadal","p/min","420","420"]
["Kompressor","Type","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10","-10"]
["","","","Max","°CDB","46","46","46"]
["","Küte","Keskkond","Min","°CWB","","","-15"]
["","","","Max","°CWB","","","24"]
["Mürarõhutase","Jahutus","","Nom","dBA","46","46","48"]
["","Küte","","Nom","dBA","47","47","48"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32"]
["","Kogus","","","kg","1.8","1.8","2"]
["","Kogus","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","25","25 (1)","25"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 30 m)","0,02 (torustikule, mille pikkus ületab 30 m)","002 (torustikule mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15.0","15.0","15"]
["","","IU - IU","Max","m","7.5","7.5","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","50","50 (2)","50"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-440"]
["Märkused","","","","","(1) - Ühe ruumi jaoks","(1) - Ühe ruumi jaoks"]
["","","","","","(2) - Mudelitega CVXM-A, FVXM-A kombineerimisel – maksimaalne torustiku pikkus on 30 m.","(2) - Mudelitega CVXM-A, FVXM-A kombineerimisel – maksimaalne torustiku pikkus on 30 m."]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor"]
["Energiatõhususe klass","","","","","","","A+++ ~ D"]