{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":8,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-G"]
[]
[]
[]
[]
["","","","","","3MXS68G3V1B2","3MXS68G3V1B","3MXS68G2V1B"]
["Mürarõhutase","Küte","","Nom","dBA","49","49"]
["","Jahutus","","Nom","dBA","48","48"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1"]
["","Tühjendusava kork","","","","1","1"]
["","Siirdmikusõlm","","","","1","1"]
["","Õhusuuna reguleerimisplaat","","","","Õhusuuna reguleerimisplaat","Õhusuuna reguleerimisplaat"]
["Jahutusaine","Charge","","","tCO2Eq","5.4","5.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Täide","","","kg","2.59","2.59"]
["","Tüüp","","","","R-410A","R-410A"]
["Torustikuühendused","Kõrguste vahe","IU - IU","Max","m","7.5","7.5"]
["","","IU - OU","Max","m","15","15"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 30 m)","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","50","50"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","936","936"]
["","","","Sügavus","mm","300","300"]
["","","","Kõrgus","mm","735","735"]
["Kaal","Ühik","","","kg","58","58"]
["Power supply","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","230","230"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","735"]
["","","","Laius","mm","","","936"]
["","","","Sügavus","mm","","","300"]
["Kaal","Ühik","","","kg","","","58"]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","","","-10"]
["","","","Max","°CDB","","","46"]
["","Küte","Keskkond","Min","°CWB","","","-15"]
["","","","Max","°CWB","","","15.5"]
["Mürarõhutase","Jahutus","","Nom","dBA","","","48"]
["","Küte","","Nom","dBA","","","49"]
["Külmaaine","Tüüp","","","","","","R-410A"]
["","Kogus","","","kg","","","2.59"]
["","Kogus","","","tCO2Eq","","","5.4"]
["","GWP","","","","","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","","25"]
["","Jahutusaine lisatäide","","","kg/m","","","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","","15"]
["","","IU - IU","Max","m","","","7.5"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","","","50"]
["Standardsed lisatarvikud","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","Air direction adjustment plate"]
["Elektritoide","Faas","","","","","","1~"]
["","Sagedus","","","Hz","","","50"]
["","Pinge","","","V","","","230"]