{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Mõõtmed","Ühik","","Kõrgus","mm","734","734"]
["","","","Laius","mm","1,040","1,040"]
["","","","Sügavus","mm","408","408"]
["Kaal","Ühik","","","kg","69","73"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10"]
["","","","Max","°CDB","46","46"]
["Mürarõhutase","Jahutus","","Nom","dBA","48","52"]
["","Küte","","Nom","dBA","49","53"]
["Külmaaine","Tüüp","","","","R-32","R-32"]
["","Kogus","","","kg","2","2.4"]
["","Kogus","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","25 (2)","25 (3)"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 30 m)","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15 (3)","15"]
["","","IU - IU","Max","m","7.5 (3)","7.5 (3)"]
["","Torustiku kogupikkus","Süsteem","Tegelikult","m","60","75"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-440","220-240"]
["Märkused","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(2) - Ühe ruumi jaoks","(2) - Ühe ruumi jaoks"]
["","","","","","(3) - Ühe ruumi jaoks (koos seadmetega FBA71/100/125 ja EKHWET ja CKHWS kasutamiseks vt kasutusjuhendit)","(3) - Ühe ruumi jaoks (koos seadmetega FBA71/100/125 ja EKHWET ja CKHWS kasutamiseks vt kasutusjuhendit)"]
["","","","","","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase"]