{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Jahutusvõimsus","Nom","","kW","9.5","12.1 (1)"]
["Ruumide jahutus","SEER","","","4.65","4.68"]
["","Aastane energiatarbimine","","kWh/a","716","1,550"]
["","Võimsus","Pdesign","kW","9.50","12.1"]
["","Energiatõhususe klass","","","B"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energiatõhususe klass","","","A"]
["","Aastane energiatarbimine","","kWh/a","2,498","3,340"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,813"]
["","Energiatõhususe suhtarv","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Energiamärgistamise direktiiv","Jahutus","","D"]
["","","Küte","","B"]
["Küttevõimsus","Nom","","kW","10.8","13.5 (2)"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(2) - Aastane elektritarbimine vastab energiamärgistuse direktiivile 2002/31/EÜ","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(3) - SEER ja SCOP vastavad standardile EN 14825","(3) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(4) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]