{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","Paigaldusjuhend"]
["","Kasutusjuhend","","","","Kasutusjuhend"]
["","Kruvi + seib","","","","Kruvi + seib"]
["","Traadita juhtimispult","","","","Traadita juhtimispult"]
["","Kattelukk, rest","","","","Kattelukk, rest"]
["","Aku","","","","Aku"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52"]
["","Gaas","","Välisdiameeter","mm","15.88"]
["","Tühjendus","","","","19.05"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.128"]
["","Küte","","Nom","kW","0.128"]
["Müratase","Jahutamine","","","dBA","64"]
["","Soojendamine","","","dBA","64"]
["Mõõtmed","Ühik","","Laius","mm","600"]
["","","","Sügavus","mm","1,007"]
["","","","Kõrgus","mm","285"]
["Korpus","Materjal","","","","Galvaanitud teras"]
["Kaal","Ühik","","","kg","35"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Madal","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Nimetus","","","","V1"]
["","Pinge","","","V","220-240"]
["Sisendvõimsus","Küte","","Nom","kW","","0.109"]
["","Jahutus","","Nom","kW","","0.109"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","","70","150","150"]
["","","","Madal","Pa","","45","111","92"]
["Korpus","Materjal","","","","","Galvaanitud teras"]
["Mõõtmed","Ühik","","Kõrgus","mm","","378","378","378"]
["","","","Laius","mm","","541","1300","1500"]
["","","","Sügavus","mm","","1045","541","541"]
["Kaal","Ühik","","","kg","","44","50","56"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","22.7","40.5","48.7"]
["","","","Nom","m³/min","","20.5","37","44"]
["","","","aeglane","m³/min","","18.3","34.8","37.9"]
["","","Küte","kiire","m³/min","","22.7","40.5","48.7"]
["","","","Nom","m³/min","","20.5","37.4","43.9"]
["","","","aeglane","m³/min","","18.3","34.8","37.9"]
["","Väline staatiline rõhk","","Nom.","Pa","","57","128","122"]
["Helivõimsustase","Jahutamine","","","dBA","","60","72","73"]
["","Soojendamine","","","dBA","","60","72","73"]
["Mürarõhutase","Jahutus","","kiire","dBA","","41","53","55"]
["","","","Nom","dBA","","38"]
["","","","aeglane","dBA","","36","50","50"]
["","Küte","","kiire","dBA","","41","53","55"]
["","","","Nom","dBA","","38"]
["","","","aeglane","dBA","","36","50","50"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","","15.88","15.9","15.9"]
["","Tühjendus","","","","","19.05"]
["Standardsed lisatarvikud","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Elektritoide","Faas","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","12.10","13.00"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","13.5","15.5"]
["Korpus","Värvus","","","","","","Galvaanitud terasplaat / värvimata","Galvaanitud terasplaat / värvimata"]
["Ventilaator","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","","37","44"]
["","","Küte","Keskmine","m³/min","","","37.4","43.9"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","","52","53"]
["","Küte","","Keskmine","dBA","","","52","53"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","","","ARCWLA","ARCWLA"]