{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Mürarõhutase","Küte","","kiire","dBA","","44","","47"]
["","","","Nom","dBA","","41","","44"]
["","","","Vaikne töö","dBA","","36","","41"]
["","","","aeglane","dBA","","38","","43"]
["","Jahutus","","Vaikne töö","dBA","","36","","41"]
["","","","aeglane","dBA","","38","","43"]
["","","","kiire","dBA","","44","","47"]
["","","","Nom","dBA","","41","","44"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","Paigaldusjuhend","","Paigaldusjuhend"]
["","Kasutusjuhend","","","","","Kasutusjuhend","","Kasutusjuhend"]
["","Kruvid","","","","","Kruvid","","Kruvid"]
["","Seib","","","","","Seib","","Seib"]
["","Traadita juhtimispult","","","","","Traadita juhtimispult","","Traadita juhtimispult"]
["","Kattelukk, rest","","","","","Kattelukk, rest","","Kattelukk, rest"]
["","Aku","","","","","Aku","","Aku"]
["Juhtsüsteemid","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","9.52","","9.52"]
["","Gaas","","Välisdiameeter","mm","","15.88","","15.88"]
["","Tühjendus","","","","","19.05","","19.05"]
["Sisendvõimsus","Jahutus","","Nom","kW","","0.094","","0.137"]
["","Küte","","Nom","kW","","0.094","","0.137"]
["Müratase","Jahutamine","","","dBA","","56","","60"]
["","Soojendamine","","","dBA","","56","","60"]
["Mõõtmed","Ühik","","Laius","mm","","820","","820"]
["","","","Sügavus","mm","","820","","820"]
["","","","Kõrgus","mm","","300","","300"]
["Korpus","Materjal","","","","","Galvaanitud teras","","Galvaanitud teras"]
["Kaal","Ühik","","","kg","","39","","39"]
["Ventilaator","Õhu vooluhulk","Küte","kiire","m³/min","","29.2","","34.0"]
["","","","aeglane","m³/min","","21.0","","26.3"]
["","","","Nom","m³/min","","24.4","","29.2"]
["","","Jahutus","aeglane","m³/min","","21.0","","26.3"]
["","","","Nom","m³/min","","24.4","","29.2"]
["","","","kiire","m³/min","","29.2","","34.0"]
["","","","Vaikne töö","m³/min","","17.6","","22.1"]
["","","Jahutus","Vaikne töö","m³/min","","17.6","","22.1"]
["Ehispaneel","Kaal","","","kg","","4","","4"]
["","Mõõtmed","","Kõrgus","mm","","82","","82"]
["","","","Sügavus","mm","","990","","990"]
["","","","Laius","mm","","990","","990"]
["","Värvus","","","","","Valge","","Valge"]
["Power supply","Faas","","","","","1~","","1~"]
["","Nimetus","","","","","V1","","V1"]
["","Sagedus","","","Hz","","50","","50"]
["","Pinge","","","V","","220-240","","220-240"]
["Ventilaator","Õhu vooluhulk","Küte","Vaikne töö","m³/min","15","","22.1"]
["Sisendvõimsus","Küte","","Nom","kW","0.067","","0.137"]
["","Jahutus","","Nom","kW","0.067","","0.137"]
["Ventilaator","Õhu vooluhulk","Jahutus","Vaikne töö","m³/min","15","","22.1"]
["Korpus","Materjal","","","","Galvaanitud teras","","Galvaanitud teras"]
["Mõõtmed","Ühik","","Kõrgus","mm","265","","300"]
["","","","Laius","mm","820","","820"]
["","","","Sügavus","mm","820","","820"]
["Kaal","Ühik","","","kg","31","","39"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","24.4","","34"]
["","","","Nom","m³/min","20.5","","29.2"]
["","","","aeglane","m³/min","17.6","","26.3"]
["","","Küte","kiire","m³/min","24.4","","34"]
["","","","Nom","m³/min","20.5","","29.2"]
["","","","aeglane","m³/min","17.6","","26.3"]
["Helivõimsustase","Jahutamine","","","dBA","54","","60"]
["","Soojendamine","","","dBA","54","","60"]
["Mürarõhutase","Jahutus","","kiire","dBA","41","","47"]
["","","","Nom","dBA","38","","44"]
["","","","aeglane","dBA","35","","43"]
["","","","Vaikne töö","dBA","32","","41"]
["","Küte","","kiire","dBA","41","","47"]
["","","","Nom","dBA","38","","44"]
["","","","aeglane","dBA","35","","43"]
["","","","Vaikne töö","dBA","32","","41"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","","9.52"]
["","Gaas","","Välisdiameeter","mm","15.88","","15.88"]
["","Tühjendus","","","","19.05","","19.05"]
["Ehispaneel","Mõõtmed","","Kõrgus","mm","82","","82"]
["","","","Laius","mm","990","","990"]
["","","","Sügavus","mm","990","","990"]
["","Kaal","","","kg","4","","4"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","ARCWLA","","ARCWLA"]
["","Juhtmega kaugjuhtimine","","","","ARCWB","","ARCWB"]
["Standardsed lisatarvikud","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Elektritoide","Faas","","","","1~","","1~"]
["","Sagedus","","","Hz","50","","50"]
["","Pinge","","","V","220-240","","220-240"]