{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Jahutusvõimsus","Nom","","kW","9.50","12.10"]
["Ruumide jahutus","SEER","","","5.10","4.83"]
["","Aastane energiatarbimine","","kWh/a","652","1,504"]
["","Võimsus","Pdesign","kW","9.50","12.10"]
["","Energiatõhususe klass","","","A"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Energiatõhususe klass","","","A"]
["","Aastane energiatarbimine","","kWh/a","2,793","3,167"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","2.27"]
["Küttevõimsus","Nom","","kW","10.80","13.50"]
["Märkused","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m","(3) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m"]