{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":11,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","150","150","150","150","150","150"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","","","","14.00"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","","","","13.50"]
["Korpus","Värvus","","","","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)"]
["","Materjal","","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["Mõõtmed","Ühik","","Kõrgus","mm","245","245","245","245","245","245"]
["","","","Laius","mm","700","700","1000","1000","1400","1400"]
["","","","Sügavus","mm","800","800","800","800","800","800"]
["Kaal","Ühik","","","kg","28","28","35","35","46","46"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","15","15","18","18","29","34"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","12.5","12.5","15","15","26","29"]
["","","","aeglane","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","","Küte","kiire","m³/min","15","15","18","18","29","34"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","12.5","12.5","15","15","26","29"]
["","","Küte","aeglane","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","Väline staatiline rõhk","","Nom.","Pa","30","30","30","30","40","50"]
["Helivõimsustase","Jahutamine","","","dBA","60","60","56","56","58","62"]
["Mürarõhutase","Jahutus","","kiire","dBA","35","35","30","30","34","37"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","32","32","28","28","32","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","29","29","25","25","30","32"]
["","Küte","","kiire","dBA","37","37","31","31","36","38"]
["Helirõhu tase","Küte","","Keskmine","dBA","34","34","28","28","33","35"]
["Mürarõhutase","Küte","","aeglane","dBA","29","29","25","25","30","32"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Tühjendus","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Tühjenduskõrgus","mm","","","","625","625","625","625","625","625"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Juhtmega kaugjuhtimine","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8"]
["","Operation manual","","","","1","1","1","","1","1"]
["","Clamps","","","","4","4","4","","4","4"]
["","Drain hose","","","","1","1","1","","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1"]
["","Screws","","","","40","40","40","","40","40"]
["","Sealing pads","","","","5","5","5","","5","5"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","50"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Märkused","","","","","","","","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele."]
["","","","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","","","1"]
["","riputuskanduri seib","","","","","","","8"]
["","Kasutusjuhend","","","","","","","1"]
["","Klambrid","","","","","","","4"]
["","Tühjendusvoolik","","","","","","","1"]
["","Liitmike isolatsioon","","","","","","","2"]
["","Tühjendusvooliku metallklamber","","","","","","","1"]
["","Kruvid","","","","","","","40"]
["","Tihenduspadjad","","","","","","","5"]