{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Mürarõhutase","Küte","","kiire","dBA","37","37","31"]
["","","","Keskmine","dBA","34","34","28"]
["","","","aeglane","dBA","29","29","25"]
["","Jahutus","","Keskmine","dBA","32","32","28"]
["","","","aeglane","dBA","29","29","25"]
["","","","kiire","dBA","35","35","30"]
["Standardsed lisatarvikud","Kasutusjuhend","","","","1","1","1"]
["","Paigaldusjuhend","","","","1","1","1"]
["","Tühjendusvoolik","","","","1","1","1"]
["","Tühjendusvooliku metallklamber","","","","1","1","1"]
["","riputuskanduri seib","","","","8","8","8"]
["","Kruvid","","","","40","40","40"]
["","Liitmike isolatsioon","","","","2","2","2"]
["","Tihenduspadjad","","","","5","5","5"]
["","Klambrid","","","","4","4","4"]
["Juhtimissüsteemid","Wired remote control","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Torustikuühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.52","12.70","12.70"]
["","Tühjendus","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Jahutamine","","","dBA","60","60","56"]
["Mõõtmed","Ühik","","Laius","mm","700","700","1,000"]
["","","","Sügavus","mm","800","800","800"]
["","","","Kõrgus","mm","245","245","245"]
["Korpus","Materjal","","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["","Värvus","","","","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)"]
["Kaal","Ühik","","","kg","28.0","28.0","35.0"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","150","150","150"]
["","","","Nom.","Pa","30","30","30"]
["","Õhu vooluhulk","Küte","kiire","m³/min","15.0","15.0","18.0"]
["","","","aeglane","m³/min","10.5","10.5","12.5"]
["","","","Keskmine","m³/min","12.5","12.5","15.0"]
["","","Jahutus","aeglane","m³/min","10.5","10.5","12.5"]
["","","","Keskmine","m³/min","12.5","12.5","15.0"]
["","","","kiire","m³/min","15.0","15.0","18.0"]
["Tühjenduskõrgus","mm","","","","625","625","625"]
["Power supply","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220"]
["Märkused","","","","","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele.","(1) - Müravõimsus vastab müraallika absoluutväärtusele."]
["","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","","","","150","150","150"]
["Korpus","Värvus","","","","","","","Värvimata (tsingitud)","Värvimata (tsingitud)","Värvimata (tsingitud)"]
["","Materjal","","","","","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","","245","245","245"]
["","","","Laius","mm","","","","1000","1400","1400"]
["","","","Sügavus","mm","","","","800","800","800"]
["Kaal","Ühik","","","kg","","","","35","46","46"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","","","18","29","34"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","","","15","26","29"]
["","","","aeglane","m³/min","","","","12.5","23","23.5"]
["","","Küte","kiire","m³/min","","","","18","29","34"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","","","15","26","29"]
["","","Küte","aeglane","m³/min","","","","12.5","23","23.5"]
["","Väline staatiline rõhk","","Nom.","Pa","","","","30","40","50"]
["Helivõimsustase","Jahutamine","","","dBA","","","","56","58","62"]
["Mürarõhutase","Jahutus","","kiire","dBA","","","","30","34","37"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","","","28","32","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","","","25","30","32"]
["","Küte","","kiire","dBA","","","","31","36","38"]
["Helirõhu tase","Küte","","Keskmine","dBA","","","","28","33","35"]
["Mürarõhutase","Küte","","aeglane","dBA","","","","25","30","32"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","","","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","","","","15.9","15.9","15.9"]
["","Tühjendus","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Tühjenduskõrgus","mm","","","","","","","625","625","625"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Juhtmega kaugjuhtimine","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardsed lisatarvikud","Installation manual","","","","","","","1","1","1"]
["","Washer for hanger bracket","","","","","","","8","8","8"]
["","Operation manual","","","","","","","1","1","1"]
["","Clamps","","","","","","","4","4","4"]
["","Drain hose","","","","","","","1","1","1"]
["","Insulation for fitting","","","","","","","2","2","2"]
["","Metal clamp for drain hose","","","","","","","1","1","1"]
["","Screws","","","","","","","40","40","40"]
["","Sealing pads","","","","","","","5","5","5"]
["Elektritoide","Faas","","","","","","","1~","1~","1~"]
["","Sagedus","","","Hz","","","","50","50","50"]
["","Pinge","","","V","","","","220-240/220","220-240/220","220-240/220"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","","","","14.00"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","","","","13.50"]