{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Mürarõhutase","Küte","kiire","dBA","37","37","31","31","36","38"]
["","","Nom","dBA","37","37","31","31","36","38"]
["","","Keskmine","dBA","34","34","28","28","33","35"]
["","","aeglane","dBA","29","29","25","25","30","32"]
["","Jahutus","Keskmine","dBA","32","32","28","28","32","35"]
["","","aeglane","dBA","29","29","25","25","30","32"]
["","","kiire","dBA","35","35","30","30","34","37"]
["","","Nom","dBA","35","35","30","30","34","37"]
["Standardsed lisatarvikud","Kasutusjuhend","","","1","1","1","1","1","1"]
["","Paigaldusjuhend","","","1","1","1","1","1","1"]
["","Tühjendusvoolik","","","1","1","1","1","1","1"]
["","Tühjendusvooliku metallklamber","","","1","1","1","1","1","1"]
["","riputuskanduri seib","","","8","8","8","8","8","8"]
["","Kruvid","","","40","40","40","40","40","40"]
["","Liitmike isolatsioon","","","2","2","2","2","2","2"]
["","Tihenduspadi","","","5","5","5","5","5","5"]
["","Klambrid","","","4","4","4","4","4","4"]
["Külmaaine","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Jahutusvõimsus","Üldvõimsus","Nom","kW","","","","","","12.10"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gaas","Välisdiameeter","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Tühjendus","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Müratase","Jahutamine","","dBA","60","60","56","56","58","62"]
["Mõõtmed","Ühik","Laius","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Sügavus","mm","800","800","800","800","800","800"]
["","","Kõrgus","mm","245","245","245","245","245","245"]
["Korpus","Materjal","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["","Värvus","","","Värvimata","Värvimata","Värvimata","Värvimata","Värvimata","Värvimata"]
["Kaal","Ühik","","kg","28.0","28.0","35.0","35","46","46"]
["Ventilaator","Väline staatiline rõhk","Kõrge","Pa","150","150","150","150","150","150"]
["","","Nom.","Pa","30","30","30","30","40","50"]
["Küttevõimsus","Üldvõimsus","Nom.","kW","","","","","","13.5"]
["Power supply","Faas","","","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","Hz","50","50","50","50","50","50"]
["","Pinge","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Märkused","","","","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele."]