{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","AHQ100CV1 / AZQS100B7Y1B UK","AHQ125CV1 / AZQS125B7Y1B UK","AHQ140CV1 / AZQS140B7Y1B UK"]
["Jahutusvõimsus","Nom","","kW","9.5","12.1","13.0"]
["Ruumide jahutus","SEER","","","4.60"]
["","Aastane energiatarbimine","","kWh/a","716"]
["","Võimsus","Pdesign","kW","9.50"]
["","Energiatõhususe klass","","","B"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","7.60"]
["","SCOP/A","","","3.80"]
["","Energiatõhususe klass","","","A"]
["","Aastane energiatarbimine","","kWh/a","2,800"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,810","2,300"]
["","Energiatõhususe suhtarv","","","2.62","2.63","3.01"]
["","COP","","","3.41","3.61","3.41"]
["","Energiamärgistamise direktiiv","Jahutus","","D","D"]
["","","Küte","","B","A"]
["Küttevõimsus","Nom","","kW","10.8","13.5","15.5"]
["Märkused","","","","(1) - Aastane elektritarbimine vastab energiamärgistuse direktiivile 2002/31/EÜ","(1) - Aastane elektritarbimine vastab energiamärgistuse direktiivile 2002/31/EÜ","(1) - Aastane elektritarbimine vastab energiamärgistuse direktiivile 2002/31/EÜ"]
["","","","","(2) - SEER ja SCOP vastavad standardile EN 14825","(2) - SEER ja SCOP vastavad standardile EN 14825","(2) - SEER ja SCOP vastavad standardile EN 14825"]
["","","","","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]