{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Sisendvõimsus","Küte","","Nom","kW","0.106","0.149"]
["","Jahutus","","Nom","kW","0.106","0.149"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","0","0","0","0"]
["","","","Madal","Pa","0","0","0","0"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","12.10","13.00"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","13.5","15.5"]
["Korpus","Värvus","","","","Valge","Valge","Valge","Valge"]
["","Materjal","","","","Galvaanitud teras","Galvaanitud teras"]
["Mõõtmed","Ühik","","Kõrgus","mm","260","260","260","285"]
["","","","Laius","mm","1320","1538","1790","1900"]
["","","","Sügavus","mm","634","634","634","680"]
["Kaal","Ühik","","","kg","38","45","65","70"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom","m³/min","21.3","27.8","31","39"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","","31","39"]
["","","","aeglane","m³/min","18.9","24.8","27.2","28.3"]
["","","Küte","kiire","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom","m³/min","21.3","27.8","30.6","39.1"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","","30.6","39.1"]
["","","Küte","aeglane","m³/min","18.9","24.8","27.2","28.3"]
["","Väline staatiline rõhk","","Nom.","Pa","0","0","0","0"]
["Helivõimsustase","Jahutamine","","","dBA","59","64","65","71"]
["","Soojendamine","","","dBA","62","64","65","71"]
["Mürarõhutase","Jahutus","","kiire","dBA","49","52","52","56"]
["","","","Nom","dBA","48","47"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","","50","53"]
["Mürarõhutase","Jahutus","","aeglane","dBA","46","46","49","46"]
["","Küte","","kiire","dBA","49","52","52","56"]
["Helirõhu tase","Küte","","Keskmine","dBA","","","50","53"]
["Mürarõhutase","Küte","","Nom","dBA","48","47"]
["","","","aeglane","dBA","46","46","49","46"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","15.88","15.88","15.9","15.9"]
["","Tühjendus","","","","19.05","19.05"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Juhtmega kaugjuhtimine","","","","ARCWB","ARCWB"]
["Standardsed lisatarvikud","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Väljavoolutoru","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]