{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARX-K"]
[]
[]
[]
[]
["","","","","","ARX20K2V1B","ARX20K5V1B9","ARX25K2V1B","ARX25K5V1B9","ARX35K2V1B","ARX35K5V1B9"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550","550","550","550","550"]
["","","","Laius","mm","658","658","658","658","658","658"]
["","","","Sügavus","mm","275","275","275","275","275","275"]
["Kaal","Ühik","","","kg","28","26","28","26","28","28"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)"]
["","","","Max","°CDB","46","46","46","46","46","46"]
["","Küte","Keskkond","Min","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max","°CWB","18","18","18","18","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","46","46","46","46","48","48"]
["","Küte","","kiire","dBA","47","47","47","47","48","48"]
["Külmaaine","Tüüp","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Kogus","","","kg","0.74","0.74","0.74","0.74","1.0","1.0"]
["","Kogus","","","tCO2Eq","1.5","1.5","1.5","1.5","2.1","2.1"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","15","15","15","15","15","15"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","12","12","12","12","12","12"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Märkused","","","","","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB","(1) - Töövahemik kombineerituna ATX-J3-ga: min 10°CDB ~ max 46°CDB"]
["Standardsed lisatarvikud","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label","","LOT10 Energy Label"]