{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Mürarõhutase","Küte","","Nom","dBA","","49.0"]
["","Jahutus","","Nom","dBA","","49.0"]
["Standardsed lisatarvikud","Tühjendusava kork","","","","","1"]
["","Paigaldusjuhend","","","","","1"]
["","Külmutusagensi täitmise silt","","","","","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","","1"]
["","Üldised ohutusmeetmed","","","","","1"]
["Külmaaine","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Kogus","","","kg","","0.76"]
["","Tüüp","","","","","R-32"]
["Töötamisvahemik","Jahutus","Keskkond","Max","°CDB","","50 (4), 46 (5)"]
["","","","Min","°CDB","","-10"]
["Piping connections","Kõrguste vahe","IU - OU","Max","m","","15"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Kompressor","Type","","","","","Hermeetiline pöördkompressor"]
["Mõõtmed","Seade","","Laius","mm","","840"]
["","","","Sügavus","mm","","350"]
["","","","Kõrgus","mm","","552"]
["Kaal","Ühik","","","kg","","32"]
["Power supply","Faas","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]
["Märkused","","","","","(1) - Võimalik ainult koos seadmetega ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(2) - Võimalik ainult koos seadmetega ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","(3) - Vt eraldi elektriandmete joonist"]
["","","","","","","(4) - Võimalik ainult koos seadmetega ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Võimalik ainult koos seadmetega ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","552"]
["","","","Laius","mm","840"]
["","","","Sügavus","mm","350"]
["Kaal","Ühik","","","kg","32"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10"]
["","","","Max","°CDB","50 (4), 46 (5)"]
["Mürarõhutase","Jahutus","","Nom","dBA","46.0"]
["","Küte","","Nom","dBA","47.0"]
["Külmaaine","Kogus","","","kg","0.76"]
["","Kogus","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Elektritoide","Sagedus","","","Hz","50"]