{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Mürarõhutase","Küte","","kiire","dBA","","","47","48"]
["","","","Nom","dBA","","52","","","49"]
["","Jahutus","","kiire","dBA","","","46","48"]
["","","","Nom","dBA","","52","","","49"]
["Standardsed lisatarvikud","Tühjendusava kork","","","","","1","1","1","1"]
["","Paigaldusjuhend","","","","","1","1","1","1"]
["","Külmutusagensi täitmise silt","","","","","1","1","","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","","1","1","","1"]
["Külmaaine","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.70","1.0","1.2","1.50"]
["","Tüüp","","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilaatori mootor","Kiirus","Jahutus","Ülimadal","p/min","","","780","780"]
["","","Küte","Ülimadal","p/min","","","740","740"]
["Töövahemik","Jahutus","Keskkond","Max","° CDB","","46","46","46","46"]
["","","","Min","° CDB","","-10","10","10","-10"]
["","Küte","Keskkond","Max","°CWB","","18","18","18","18"]
["","","","Min","°CWB","","-15","-15","-15","-15"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","","20.0","15","15","20.0"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Müratase","Jahutamine","","","dBA","","65","","","62"]
["","Soojendamine","","","dBA","","65","","","62"]
["Kompressor","Tüüp","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","","825","765","765","825"]
["","","","Sügavus","mm","","300","285","285","300"]
["","","","Kõrgus","mm","","735","550","550","735"]
["Kaal","Ühik","","","kg","","47","34","34","47"]
["Ventilaator","Õhu vooluhulk","Küte","Ülimadal","cfm","","","904","904"]
["","","","Ülimadal","m³/min","","","25.6","25.6"]
["","","Jahutus","Ülimadal","m³/min","","","30.1","30.1"]
["","","","Ülimadal","cfm","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Sagedus","","","Hz","","50","50","50","50"]
["","Pinge","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Märkused","","","","","(1) - 220V","","(1) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid.","(1) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid."]
["","","","","","(2) - 230 V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230 V","(3) - 230 V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Sisaldav fluoritud kasvuhoonegaase","(5) - Sisaldav fluoritud kasvuhoonegaase"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","48.9"]
["","","Soojendamine","Ülimadal","m³/min","43.1"]
["","","","Ülimadal","cfm","1727"]
["","","Soojendamine","Ülimadal","cfm","1522"]
["Mõõtmed","Ühik","","Kõrgus","mm","735"]
["","","","Laius","mm","825"]
["","","","Sügavus","mm","300"]
["Kaal","Ühik","","","kg","47"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","670"]
["","","Soojendamine","Ülimadal","p/min","670"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","10"]
["","","","Max","° CDB","46"]
["","Küte","Keskkond","Min","°CWB","-15"]
["","","","Max","°CWB","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","48"]
["","Küte","","kiire","dBA","48"]
["Külmaaine","Tüüp","","","","R-410A"]
["","Kogus","","","kg","1.7"]
["","Kogus","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","20"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","","(1) - Sisaldav fluoritud kasvuhoonegaase","","","(1) - Sisaldav fluoritud kasvuhoonegaase"]