{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Helirõhu tase","Küte","","kiire","dBA","","48"]
["","","","aeglane","dBA","","45"]
["Standardsed lisatarvikud","1","","","","","550"]
["Jahutusaine","Kogus","","","kg","","2.5"]
["","Tüüp","","","","","1.2"]
["Ventilaator","Õhu voolukiirus","Jahutus","Ülimadal","m³/min","","30.1"]
["","","","Ülimadal","cfm","","1,063"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","","740"]
["","","Küte","Ülimadal","p/min","","-15"]
["Töötamisvahemik","Küte","Keskkond","Min","°CWB","","20"]
["","","","Max","°CWB","","10"]
["Helirõhu tase","Jahutus","","aeglane","dBA","","44"]
["","","","kiire","dBA","","48"]
["Kompressor","Type","","","","","Hermeetiline pöördkompressor"]
["Mõõtmed","Seade","","Laius","mm","","285"]
["","","","Sügavus","mm","","612"]
["","","","Kõrgus","mm","","765"]
["Kaal","Ühik","","","kg","","34"]
["Ventilaator","Õhu voolukiirus","Küte","Ülimadal","cfm","","904"]
["","","","Ülimadal","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]
["Märkused","","","","","(1) - 220V","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(2) - 230 V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230 V"]
["","","","","","","(4) - 240V"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","30.1"]
["","","Soojendamine","Ülimadal","m³/min","25.6"]
["","","","Ülimadal","cfm","1063"]
["","","Soojendamine","Ülimadal","cfm","904"]
["Mõõtmed","Ühik","","Kõrgus","mm","550"]
["","","","Laius","mm","765"]
["","","","Sügavus","mm","285"]
["Kaal","Ühik","","","kg","34"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","780"]
["","","Soojendamine","Ülimadal","p/min","740"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","10"]
["","","","Max","° CDB","46"]
["","Küte","Keskkond","Min","°CWB","-15"]
["","","","Max","°CWB","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","46"]
["","Küte","","kiire","dBA","47"]
["","","","aeglane","dBA","44"]
["Külmaaine","Tüüp","","","","R-410A"]
["","Kogus","","","kg","1.0"]
["","Kogus","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]