{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-J3 / ARX-K"]
[]
[]
[]
[]
["","","","","ATX20J3V1B / ARX20K2V1B","ATX20J3V1B / ARX20K5V1B9","ATX25J3V1B / ARX25K2V1B","ATX25J3V1B / ARX25K5V1B9","ATX35J3V1B / ARX35K2V1B","ATX35J3V1B / ARX35K5V1B9"]
["Jahutusvõimsus","Min","","kW","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max","","kW","2.6","2.6","3.0","3.0","3.8","3.8"]
["","Nom","","kW","2.0 (2)","2.0 (2)","2.5 (2)","2.5 (2)","3.3 (2)","3.3 (2)"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaas","Välisdiameeter","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Tühjendus","OD","mm","18","18","18","18","18","18"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","244","244","352","352","514","514"]
["","Energiatõhususe suhtarv","","","4.09 (1)","4.09 (1)","3.55 (1)","3.55 (1)","3.21 (1)","3.21 (1)"]
["","COP","","","4.24 (1)","4.24 (1)","4.06 (1)","4.06 (1)","3.76 (1)","3.76 (1)"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A","A","A","A","A"]
["","","Küte","","A","A","A","A","A","A"]
["Küttevõimsus","Nom","","kW","2.5 (2)","2.5 (2)","2.8 (2)","2.8 (2)","3.5 (2)","3.5 (2)"]
["","Min","","kW","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max","","kW","3.5","3.5","4.0","4.0","4.8","4.8"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]