{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Mürarõhutase","Küte","","kiire","dBA","","","","","","43"]
["","","","Keskmine","dBA","","","","","","35"]
["","","","Vaikne töö","dBA","","","","","","26"]
["","","","aeglane","dBA","","","","","","29"]
["","Jahutus","","Keskmine","dBA","","","","","","34"]
["","","","Vaikne töö","dBA","","","","","","20"]
["","","","aeglane","dBA","","","","","","27"]
["","","","kiire","dBA","","","","","","43"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","","","","","1"]
["","Kasutusjuhend","","","","","","","","","1"]
["","Infrapunaühendusega kaugjuhtimispult","","","","","","","","","1"]
["","AA kuivelement patareid","","","","","","","","","2"]
["","Kaugjuhtimispuldi hoidik","","","","","","","","","1"]
["","Paigaldusplaat","","","","","","","","","1"]
["","Titaanapatiidist fotokatalüütiline õhupuhastusfilter","","","","","","","","","2"]
["","Siseseadme kinnituskruvid","","","","","","","","","2"]
["Juhtimissüsteemid","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Torustikuühendused","Vedelik","","Välisdiameeter","mm","","","","","","6.35"]
["","Gaas","","Välisdiameeter","mm","","","","","","9.50"]
["","Tühjendus","","","","","","","","","18"]
["Sisendvõimsus","Jahutus","","Nom","kW","","","","","","0.024"]
["","Küte","","Nom","kW","","","","","","0.029"]
["Sound power level","Jahutamine","","","dBA","","","","","","58"]
["","Soojendamine","","","dBA","","","","","","58"]
["Mõõtmed","Ühik","","Laius","mm","","","","","","770"]
["","","","Sügavus","mm","","","","","","225"]
["","","","Kõrgus","mm","","","","","","286"]
["Korpus","Värvus","","","","","","","","","Valge"]
["Kaal","Ühik","","","kg","","","","","","9.0"]
["Power supply","Faas","","","","","","","","","1~"]
["","Sagedus","","","Hz","","","","","","50"]
["","Nimetus","","","","","","","","","V1"]
["","Pinge","","","V","","","","","","220-240"]
["Märkused","","","","","","","","","","(1) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.018","0.018","0.02","0.02","0.024"]
["","Küte","","Nom","kW","0.022","0.022","0.023","0.023","0.029"]
["Korpus","Värvus","","","","Valge","Valge","Valge","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","286","286","286","286","286"]
["","","","Laius","mm","770","770","770","770","770"]
["","","","Sügavus","mm","225","225","225","225","225"]
["Kaal","Ühik","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","7.8","7.8","8","8","8.2"]
["","","","aeglane","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Vaikne töö","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Küte","kiire","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","Küte","aeglane","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Vaikne töö","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Helivõimsustase","Jahutamine","","","dBA","55","55","55","55","58"]
["","Soojendamine","","","dBA","55","55","55","55","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","39","39","40","40","43"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","33","33","33","33","34"]
["Mürarõhutase","Jahutus","","aeglane","dBA","25","25","26","26","27"]
["","","","Vaikne töö","dBA","20","20","20","20","20"]
["","Küte","","kiire","dBA","39","39","40","40","43"]
["Helirõhu tase","Küte","","Keskmine","dBA","34","34","34","34","35"]
["Mürarõhutase","Küte","","aeglane","dBA","28","28","28","28","29"]
["","","","Vaikne töö","dBA","23","23","23","23","26"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5","9.5","9.5","9.5"]
["","Tühjendus","","","","18","18","18","18","18"]
["Juhtimissüsteemid","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Elektritoide","Nimetus","","","","V1","V1","V1","V1","V1"]
["","Faas","","","","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardsed lisatarvikud","AAA dry-cell batteries","","","","","2","","2","2"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","","","ARC480A11","ARC480A11"]
["Standardsed lisatarvikud","Titanium apatite photocatalytic air purification filter","","","","","","2"]