{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Mürarõhutase","Küte","kiire","dBA","41","41"]
["","","Vaikne töö","dBA","26","26"]
["","","aeglane","dBA","29","29"]
["","Jahutus","Vaikne töö","dBA","23","23"]
["","","aeglane","dBA","27","27"]
["","","kiire","dBA","41","41"]
["","","Nom","dBA","35","35"]
["","Jahutus","Nom","dBA","34","34"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","1","1"]
["","Kasutusjuhend","","","1","1"]
["","Infrapunaühendusega kaugjuhtimispult","","","1","1"]
["","Akud","","","2","2"]
["","Kaugjuhtimispuldi hoidik","","","1","1"]
["","Paigaldusplaat","","","1","1"]
["","Titaanapatiidist fotokatalüütiline õhupuhastusfilter","","","2","2"]
["","Siseseadme kinnituskruvid","","","2","2"]
["Juhtsüsteemid","Infrared remote control","","","ARC433A87","ARC433A87"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","Välisdiameeter","mm","9.5","9.5"]
["","Drain","","","18","18"]
["Power input","Jahutus","Nom","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Küte","Nom","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Sound power level","Jahutamine","","dBA","57","57"]
["","Soojendamine","","dBA","57","57"]
["Mõõtmed","Ühik","Laius","mm","770","770"]
["","","Sügavus","mm","198","198"]
["","","Kõrgus","mm","283","283"]
["Korpus","Värvus","","","Valge","Valge"]
["Kaal","Ühik","","kg","8","8"]
["Power supply","Faas","","","1~","1~"]
["","Sagedus","","Hz","50","50"]
["","Nimetus","","","V1","V1"]
["","Pinge","","V","220-240","220-240"]
["Märkused","","","","(1) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid.","(1) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240V","(4) - 240V"]