{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Jahutusvõimsus","Min","","kW","","","1.40"]
["","Max","","kW","","","4.00"]
["","Nom","","kW","","","3.40"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","","","402"]
["","Energiatõhususe suhtarv","","","","","4.23"]
["","COP","","","","","4.04"]
["","Energiamärgistamise direktiiv","Jahutus","","","","A"]
["","","Küte","","","","A"]
["Küttevõimsus","Nom","","kW","","","4.00"]
["","Min","","kW","","","1.40"]
["","Max","","kW","","","5.20"]
["Märkused","","","","","","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","","(3) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Jahutusvõimsus","Min","","kW","1.30","1.30","","1.40"]
["","Nom","","kW","2.50","2.50","","3.40"]
["","Max","","kW","3.20","3.20","","4.00"]
["Küttevõimsus","Min","","kW","1.30","1.30","","1.40"]
["","Nom","","kW","2.80","2.80","","4.00"]
["","Max","","kW","4.70","4.70","","5.20"]
["Nimikasutegur","Energiatõhususe suhtarv","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Aastane energiatarve","","kWh","278","278","","402"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A","","A"]
["","","Küte","","A","A","","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A+++","A+++","","A+++"]
["","Võimsus","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Aastane energiatarbimine","","kWh/a","102","102","","139"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A+++","A+++","","A+++"]
["","Võimsus","Pdesign","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.30","2.30","","2.35"]
["","Aastane energiatarbimine","","kWh/a","659","659","","686"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]