{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Jahutusvõimsus","Nom","","kW","","2.50","3.50"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Energiamärgistamise direktiiv","Jahutus","","","A","A"]
["","","Küte","","","A","A"]
["Küttevõimsus","Nom","","kW","","3.00","4.00"]
["Märkused","","","","","(1) - Jahutus: T2: ruumitemp. 26,6 °CDB, 19,4 °CWB, välistemp. 48°CDB [Btu/hr/W]","(1) - Jahutus: T2: ruumitemp. 26,6 °CDB, 19,4 °CWB, välistemp. 48°CDB [Btu/hr/W]"]
["","","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]
["Outdoor unit","","","","ARXP20K3V1B"]
["Jahutusvõimsus","Nom","","kW","2.00"]
["Küttevõimsus","Nom","","kW","2.50"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.98"]
["","COP","","","4.77"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A++"]
["","Võimsus","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Aastane energiatarbimine","","kWh/a","104"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A++"]
["","Võimsus","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.19"]
["","Aastane energiatarbimine","","kWh/a","664"]