{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.019","0.020","0.032"]
["","Küte","","Nom","kW","0.023","0.023","0.032"]
["Korpus","Colour","","","","Valge","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","286","286","286"]
["","","","Laius","mm","770","770","770"]
["","","","Sügavus","mm","225","225","225"]
["Kaal","Ühik","","","kg","8.50","8.50","9.00"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","9.5","9.7","11.5"]
["","","","Keskmine","m³/min","7.4","7.7","8.3"]
["","","","aeglane","m³/min","5.6","5.8","6.3"]
["","","","Vaikne töö","m³/min","4.2","4.2","4.5"]
["","","Küte","kiire","m³/min","10.4","10.4","11.5"]
["","","","Keskmine","m³/min","8.1","8.1","9.0"]
["","","","aeglane","m³/min","6.2","6.4","7.0"]
["","","","Vaikne töö","m³/min","5.2","5.2","5.1"]
["Müratase","Jahutamine","","","dBA","55","55","58"]
["","Soojendamine","","","dBA","55","55","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","39","40","43"]
["","","","Keskmine","dBA","33","33","34"]
["","","","aeglane","dBA","25","26","27"]
["","","","Vaikne töö","dBA","19","19","20"]
["","Küte","","kiire","dBA","39","40","40"]
["","","","Keskmine","dBA","34","34","35"]
["","","","aeglane","dBA","28","28","29"]
["","","","Vaikne töö","dBA","21","21","21"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6","6","6"]
["","Gaas","","Välisdiameeter","mm","9.50","9.50","9.50"]
["","Tühjendus","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1","1"]
["","Kasutusjuhend","","","","1","1","1"]
["","Infrapunaühendusega kaugjuhtimispult","","","","1","1","1"]
["","AAA kuivelement patareid","","","","2","2","2"]
["","Kaugjuhtimispuldi hoidik","","","","1","1","1"]
["","Paigaldusplaat","","","","1","1","1"]
["","Titaanapatiidist deodoriseeriv filter","","","","1","1","1"]
["","Hõbedaioonidega filter","","","","1","1","1"]
["","Siseseadme kinnituskruvid","","","","2","2","2"]
["","Üldised ohutusmeetmed","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m (horisontaalne)","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m (horisontaalne)","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m (horisontaalne)"]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]