{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.03","0.03"]
["","Küte","","Nom","kW","0.035","0.035"]
["Korpus","Värvus","","","","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","285","285"]
["","","","Laius","mm","770","770"]
["","","","Sügavus","mm","225","225"]
["Kaal","Ühik","","","kg","9","9"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","10.6","11.4"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","7.7","8.2"]
["","","","aeglane","m³/min","5.3","5.4"]
["","","","Vaikne töö","m³/min","4.3","4.3"]
["","","Küte","kiire","m³/min","11.2","10.8"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","8","7.8"]
["","","Küte","aeglane","m³/min","5.8","5.8"]
["","","","Vaikne töö","m³/min","4.9","4.9"]
["Helivõimsustase","Jahutamine","","","dBA","58","58"]
["","Soojendamine","","","dBA","58","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","43","43"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","35","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","26","26"]
["","","","Vaikne töö","dBA","21","21"]
["","Küte","","kiire","dBA","43","43"]
["Helirõhu tase","Küte","","Keskmine","dBA","35","35"]
["Mürarõhutase","Küte","","aeglane","dBA","26","26"]
["","","","Vaikne töö","dBA","21","21"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5"]
["","Tühjendus","","","","16 (ühendusvooliku sisemine läbimõõt)","16 (ühendusvooliku sisemine läbimõõt)"]
["Juhtimissüsteemid","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Elektritoide","Nimetus","","","","V1","V1"]
["","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]