{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BPMKS967A"]
[]
[]
[]
[]
["","","","","","BPMKS967B2B","BPMKS967B3B"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1"]
["","Siirdmik välisseadme poolele; gaasitoru läbimõõt 12,7","","","","1","1"]
["","Siirdmik välisseadme poolele; gaasitoru läbimõõt 15,9","","","","1","1"]
["","Siirdmik välisseadme poolele; gaasitoru läbimõõt 19,1","","","","1","1"]
["","Siirdmik välisseadme poolele; vedelikutoru läbimõõt 6,4","","","","1","1"]
["","Siirdmik siseseadme poolele; gaasitoru läbimõõt 9,52","","","","1","1"]
["","Siirdmik siseseadme poolele; vedelikutoru läbimõõt 12,7","","","","2","3"]
["","Siirdmik siseseadme poolele; vedelikutoru läbimõõt 9,5","","","","2","3"]
["","Metallist riputi","","","","4","4"]
["","Kruvid (M4x8)","","","","8","8"]
["","Soojusisolatsioon","","","","3","4"]
["","Kinnitusriba","","","","2","2"]
["Mõõtmed","Ühik","","Laius","mm","650","650"]
["","","","Sügavus","mm","350","350"]
["","","","Kõrgus","mm","180","180"]
["Kaal","Ühik","","","kg","7.5","8"]
["Ühendatava siseseadme tüüp","","","","","20 klass - 71 klass","20 klass - 71 klass"]
["Torustikuühendused","Välisseade","Vedelik","Kogus","","1","1"]
["","","","ID","mm","9.5","9.5"]
["","","Gaas","Kogus","mm","1","1"]
["","","","ID","mm","19.1","19.1"]
["","Siseseade","Gaas","Kogus","mm","2","3"]
["","","","ID","mm","15.9","15.9"]
["","","Vedelik","ID","mm","6.4","6.4"]
["","","","Kogus","","2","3"]
["","Tühjendus","","ID","mm","Töötluseta tühjendus","Töötluseta tühjendus"]
["Sisendvõimsus","Nom.","","","kW","0.010","0.010"]
["Power supply","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","230","230"]