{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52W"]
[]
[]
[]
[]
["","","","","BRC1H52W."]
["Pakend","Materjal","","","Papp"]
["","Kaal","","kg","0.0850"]
["Välistemperatuur","Suhteline niiskus <","","%","95"]
["","Säilitamine","Min","°C","-20"]
["","","Max","°C","70"]
["","Kasutus","Min","°C","-10"]
["","","Max","°C","50"]
["Mõõtmed","Pakitud seade","Laius","mm","217"]
["","","Kõrgus","mm","50"]
["","","Sügavus","mm","161"]
["","Ühik","Laius","mm","85"]
["","","Sügavus","mm","25"]
["","","Kõrgus","mm","85"]
["Korpus","Nupukate","","","Ei"]
["","Värvus","","","Valge"]
["","Talitlus-LED","Värvus","","Blue status indicator"]
["LCD","Tüüp","","","100 x 150 dots"]
["","Tagantvalgustus","Värvus","","Valge"]
["","Mõõtmed","Laius","mm","28.0"]
["","","Kõrgus","mm","40.7"]
["Kaal","Pakitud seade","","kg","0.317"]
["","Ühik","","kg","0.110"]
["Elektriühendused","Juhtmepikkus","Max","m","500"]