{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Korpus","Värvus","","","Valge"]
["","Nupukate","","","Ei"]
["","Talitlus-LED","Värvus","","Sinine olekuindikaator"]
["Mõõtmed","Ühik","Kõrgus","mm","85"]
["","","Laius","mm","85"]
["","","Sügavus","mm","25"]
["","Pakitud seade","Kõrgus","mm","50"]
["","","Laius","mm","217"]
["","","Sügavus","mm","161"]
["Kaal","Ühik","","kg","0.110"]
["","Pakitud seade","","kg","0.317"]
["Pakend","Materjal","","","Papp"]
["","Kaal","","kg","0.0850"]
["LCD","Tüüp","","","100 x 150 punkti"]
["","Mõõtmed","Kõrgus","mm","40.7"]
["","","Laius","mm","28.0"]
["","Tagantvalgustus","Värvus","","Valge"]
["Keskkonna temperatuur","Kasutus","Min","°C","-10"]
["","","Max","°C","52"]
["","Säilitamine","Min","°C","-20"]
["","","Max","°C","70"]
["","Keskkonna temperatuur-=-Suhteline niiskus <-=-%","","%","95"]
["Juhtimissüsteemid","Temperatuurijuhtimise klass","","","VI"]
["","Panus kütmise sesoonsesse kasutegurisse","","%","4.0"]
["Elektriühendused","Juhtmepikkus","Max","m","500"]