{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.020"]
["","Küte","","Nom","kW","0.020"]
["Korpus","Värvus","","","","Must"]
["Mõõtmed","Ühik","","Kõrgus","mm","295"]
["","","","Laius","mm","798"]
["","","","Sügavus","mm","189"]
["Kaal","Ühik","","","kg","11.5"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","11.0"]
["","","","Keskmine","m³/min","8.2"]
["","","","aeglane","m³/min","6.1"]
["","","","Vaikne töö","m³/min","4.6"]
["","","Küte","kiire","m³/min","10.9"]
["","","","Keskmine","m³/min","8.7"]
["","","","aeglane","m³/min","6.4"]
["","","","Vaikne töö","m³/min","4.5"]
["Sound power level","Jahutamine","","","dBA","57"]
["Mürarõhutase","Jahutus","","kiire","dBA","39"]
["","","","Keskmine","dBA","32"]
["","","","aeglane","dBA","25"]
["","","","Vaikne töö","dBA","21"]
["","Küte","","kiire","dBA","39"]
["","","","Keskmine","dBA","32"]
["","","","aeglane","dBA","25"]
["","","","Vaikne töö","dBA","21"]
["Jahutusaine","GWP","","","","675.0"]
["Torustikuühendused","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.50"]
["","Tühjendus","","","","18"]
["Juhtimissüsteemid","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kasutusjuhend","","","","1"]
["","Õhufilter","","","","2"]
["","Infrapunaühendusega kaugjuhtimispult","","","","1"]
["","Kaugjuhtimispuldi paigaldusplaat","","","","1"]
["","Kruvide kott","","","","1"]
["","Kruvide kaas","","","","2"]
["","AAA kuivelement patareid","","","","2"]
["","Üldised ohutusmeetmed","","","","1"]
["Power supply","Nimetus","","","","V1"]
["","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]