{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 5MXM-N9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / FTXM71R2V1B / 5MXM90N2V1B9","CTXM15R5V1B / FTXM71R2V1B / 5MXM90N2V1B9"]
["Jahutusvõimsus","Nom","","kW","8.00","8.00"]
["Ruumide jahutus","SEER","","","6.84","6.84"]
["","Aastane energiatarbimine","","kWh/a","410","410"]
["","Võimsus","Pdesign","kW","8.00","8.00"]
["","Energiatõhususe klass","","","A+++","A+++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","4.28","4.28"]
["","Energiatõhususe klass","","","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","1,472","1,472"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,202","1,202"]
["","Energiatõhususe suhtarv","","","3.33","3.33"]
["","COP","","","3.67","3.67"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Küttevõimsus","Nom","","kW","10.00","10.00"]
["Märkused","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]