{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Helirõhu tase","Küte","","kiire","dBA","38","","41"]
["","","","Vaikne töö","dBA","21","","21"]
["","","","aeglane","dBA","28","","30"]
["","Jahutus","","Vaikne töö","dBA","21","","21"]
["","","","aeglane","dBA","25","","28"]
["","","","kiire","dBA","37","","42"]
["","","","Nom","dBA","33"]
["","Jahutus","","Nom","dBA","31","","35"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","","1"]
["","Kasutusjuhend","","","","1","","1"]
["","Traadita juhtimispult","","","","1","","1"]
["","Akud","","","","2","","2"]
["","Kaugjuhtimispuldi hoidik","","","","1","","1"]
["","Paigaldusplaat","","","","1","","1"]
["","Siseseadme kinnituskruvid","","","","2","","2"]
["","Titaanapatiidist fotokatalüütiline õhupuhastusfilter","","","","2","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","","9.5"]
["","Drain","","","","18","","18"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.040","","0.040"]
["","Küte","","Nom","kW","0.040","","0.040"]
["Müratase","Jahutamine","","","dBA","55","","59"]
["","Soojendamine","","","dBA","56","","58"]
["Mõõtmed","Ühik","","Laius","mm","780","","780"]
["","","","Sügavus","mm","215","","215"]
["","","","Kõrgus","mm","289","","289"]
["Korpus","Colour","","","","Valge","","Valge"]
["Kaal","Ühik","","","kg","8","","8"]
["Ventilaator","Õhu voolukiirus","Küte","kiire","m³/min","","","10.1"]
["","","","aeglane","m³/min","","","6.3"]
["","","","Vaikne töö","m³/min","","","4.3"]
["","","Jahutus","aeglane","m³/min","","","5.2"]
["","","","kiire","m³/min","","","9.2"]
["","","","Vaikne töö","m³/min","","","3.9"]
["","","","Nom","m³/min","","","8.1"]
["","","Jahutus","Nom","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Sagedus","","","Hz","50","","50"]
["","Nimetus","","","","V1","","V1"]
["","Pinge","","","V","220-240","","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Sisendvõimsus","Jahutus","","Nom","kW","","0.04","","0.040"]
["","Küte","","Nom","kW","","0.04","","0.040"]
["Korpus","Värvus","","","","","Valge","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","","289","","289"]
["","","","Laius","mm","","780","","780"]
["","","","Sügavus","mm","","215","","215"]
["Kaal","Ühik","","","kg","","8","","8.00"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","7.9","","9.2"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","6.3","","7.2"]
["","","","aeglane","m³/min","","4.7","","5.2"]
["","","","Vaikne töö","m³/min","","3.9","","3.9"]
["","","Küte","kiire","m³/min","","9","","10.1"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","7.5","","8.1"]
["","","Küte","aeglane","m³/min","","6","","6.3"]
["","","","Vaikne töö","m³/min","","4.3","","4.3"]
["Helivõimsustase","Jahutamine","","","dBA","","55","","59"]
["","Soojendamine","","","dBA","","56","","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","","37","","42"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","31","","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","25","","28"]
["","","","Vaikne töö","dBA","","21","","21"]
["","Küte","","kiire","dBA","","38","","41"]
["Helirõhu tase","Küte","","Keskmine","dBA","","33","","36"]
["Mürarõhutase","Küte","","aeglane","dBA","","28","","30"]
["","","","Vaikne töö","dBA","","21","","21"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","6.35","","6.35"]
["","Gaas","","Välisdiameeter","mm","","9.5","","9.50"]
["","Tühjendus","","","","","18","","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardsed lisatarvikud","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Elektritoide","Nimetus","","","","","V1","","V1"]
["","Faas","","","","","1~","","1~"]
["","Sagedus","","","Hz","","50","","50"]
["","Pinge","","","V","","220-240","","220-240"]