{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Keskkonna temperatuur","Suhteline niiskus <","","","%","85"]
["Ühendatavate siseseadmete suurim arv","","","","","32"]
["Sisendvõimsus","kW","","","","0.015 (1)"]
["Side","DIII-NET","","Kogus","","1"]
["","","","Märkus","","DIII-NET (F1F2)"]
["","Ethernet","","Kogus","","1"]
["","Sisendklemm","Digitaalne","Kogus","","4"]
["Mõõtmed","Seade","","Laius","mm","384"]
["","","","Sügavus","mm","92"]
["","","","Kõrgus","mm","136"]
["Ühendatavate välisseadmete suurim arv","","","","","7"]
["Power supply","Sagedus","","","Hz","50/60"]
["","Pinge","","","V","110-240 VV"]
["Märkused","","","","","(1) - Hõlmab WAGO toiteallika, protsessori mooduli ja sisend-väljundmooduli toitesisendi"]
["","","","","","(2) - Mõõtmed hõlmavad WAGO toiteallika, protsessori mooduli, sisend-väljundmooduli ja vajaliku vahemaa erinevate osade vahel"]
["","","","","","(3) - Valikvarustusse kuuluva ekraani mõõtmed on järgmised: kõrgus: 209 mm, laius: 123 mm, sügavus: 8,5 mm"]