{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-D3"]
[]
[]
[]
[]
["","","","","","EHSH04P30DA3","EHSH08P50DA3","EHSH08P30DA3"]
["Korpus","Värvus","","","","Valge (RAL9016) / tumehall (RAL7011)","Valge (RAL9016) / tumehall (RAL7011)","Valge (RAL9016) / tumehall (RAL7011)"]
["","Materjal","","","","Löögikindel polüpropüleen","Löögikindel polüpropüleen","Löögikindel polüpropüleen"]
["Mõõtmed","Ühik","","Kõrgus","mm","1891","1896","1891"]
["","","","Laius","mm","595","790","595"]
["","","","Sügavus","mm","615","790","615"]
["Kaal","Ühik","","","kg","73.0","93.0","73.0"]
["PED","Kategooria","","","","art. 3.3","art. 3.3","art. 3.3"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Kogus","","","kg","1.50","1.50","1.50"]
["Müratase","Nom","","","dBA","39","39","39"]
["Töövahemik","Küte","Vee pool","Min","°C","18","18","18"]
["","","","Max","°C","65","65","65"]
["","Jahutus","Keskkond","Min","°CDB","10","10","10"]
["","","Vee pool","Min","°C","5","5","5"]
["","","","Max","°C","22","22","22"]
["Elektritoide","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","230","230","230"]
["Elektriline küttekeha","Elektritoide","","Nimetus","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Faas","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Sagedus","Hz","50","50","50"]
["Märkused","","","","","(1) - Soojuskadu vastab standardile EN12897","(1) - Soojuskadu vastab standardile EN12897","(1) - Soojuskadu vastab standardile EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃"]
["","","","","","","(5) - Kuumutage mahutit ainult soojuspumbaga, mitte elektrilise küttekehaga"]