{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3 / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3 / ERGA04EAV3"]
["Tarbevee soojendamine","Üldteave","","Esitatud koormusprofiil","","L"]
["","Keskmine kliima","","Vee soojendamise energiatõhususe klass","","A+"]
["COP","","","","","5.10 (1), 3.65 (2)"]
["Siseseade","","","","","EHSHB04P30DA3"]
["Ruumiküte","Vee väljalase 55°C keskmises kliimas","Üldteave","Seasonal space heating eff. class","","A++"]
["","","","ηs (ruumikütte sesoonne tõhusus)","%","127"]
["","","","SCOP","","3.26"]
["Küttevõimsus","Nom","","","kW","4.30 (1), 4.60 (2)"]
["Sisendvõimsus","Küte","","Nom","kW","0.840 (1), 1.26 (2)"]
["Märkused","","","","","(1) - Tingimus 1: jahutus Ta 35 °C - LWE 18°C (DT = 5°C); kütmine Ta DB/WB 7 °C / 6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Tingimus 2: jahutus Ta 35 °C - LWE 7°C (DT = 5°C); kütmine Ta DB/WB 7 °C / 6 °C - LWC 45°C (DT = 5 °C)"]