{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EA6VG / ERGA04EAV37","EHVX04S18EA6VG / ERGA04EAV37"]
["Küttevõimsus","Nom","","","kW","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)"]
["Jahutusvõimsus","Nom","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Sisendvõimsus","Küte","","Nom","kW","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)"]
["","Jahutus","","Nom","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["","Soe tarbevesi vahemikus 10°C kuni 50 °C","","Nom","kWh","3.01","2.48"]
["Soojendusaeg temperatuurilt 10°C temperatuurini 50 °C","t","","","","1h40min","1h28min"]
["COP","","","","","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Tarbevee soojendamine","Üldteave","","Esitatud koormusprofiil","","XL","L"]
["","Keskmine kliima","","Vee soojendamise energiatõhususe klass","","A","A"]
["Ruumiküte","Vee väljalase 55°C keskmises kliimas","Üldteave","SCOP","","3.29","3.29"]
["","","","Ruumikütte sesoonse tõhususe klass","","A++","A++"]
["","Vee väljalase 35°C keskmises kliimas","Üldteave","SCOP","","4.96","4.96"]
["","","","Ruumikütte sesoonse tõhususe klass","","A+++","A+++"]
["Energiatõhususe klass","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Märkused","","","","","(1) - Tingimus 1: jahutus Ta 35 °C - LWE 18°C (DT = 5°C); kütmine Ta DB/WB 7°C / 6°C - LWC 35°C (DT = 5°C)","(1) - Tingimus 1: jahutus Ta 35 °C - LWE 18°C (DT = 5°C); kütmine Ta DB/WB 7°C / 6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Tingimus 2: jahutus Ta 35 °C - LWE 7°C (DT = 5°C); kütmine Ta DB/WB 7°C / 6°C - LWC 45°C (DT = 5°C)","(2) - Tingimus 2: jahutus Ta 35 °C - LWE 7°C (DT = 5°C); kütmine Ta DB/WB 7°C / 6°C - LWC 45°C (DT = 5°C)"]