{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Mõõtmed","Ühik","","Kõrgus","mm","740"]
["","","","Laius","mm","884"]
["","","","Sügavus","mm","388"]
["Kaal","Ühik","","","kg","58.5"]
["Töövahemik","Jahutus","","Min","°CDB","10"]
["","","","Max","°CDB","43"]
["","Kuum tarbevesi","","Min","°CDB","-25"]
["","Soe tarbevesi","","Max","°CDB","35"]
["Müratase","Küte","","Nom","dBA","60 (1)"]
["","Jahutus","","Nom","dBA","62 (1)"]
["Mürarõhutase","Küte","","Nom","dBA","47 (1)"]
["","Jahutus","","Nom","dBA","49 (1)"]
["Külmaaine","Tüüp","","","","R-32"]
["","GWP","","","","675.0"]
["","Kogus","","","tCO2Eq","1.01"]
["","Kogus","","","kg","1.50"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6"]
["","Gaas","","Välisdiameeter","mm","15.9"]
["Torustikuühendused","Tühjendus","","OD","mm","18"]
["","Kõrguste vahe","IU - OU","Max","m","30.0"]
["Toruühendused","Soojusisolatsioon","","","","Nii vedeliku- kui gaasitorud"]
["Elektritoide","Nimetus","","","","V3"]
["","Faas","","","","1N~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","230"]
["Vool","Vool-=-Soovitatavad kaitsmed-=-A","","","A","20"]
["Märkused","","","","","(1) - Jahutus Ta 35 °C - LWE 18 °C (DT = 5 °C); Küte Ta DB/WB 7 °C / 6 °C - LWC 35 °C (DT = 5 °C)"]