{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":10,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWWS-VZPS"]
[]
[]
[]
[]
["","","","","EWWS500VZPSA1","EWWS710VZPSA1","EWWS900VZPSA1","EWWSC12VZPSA2","EWWSC16VZPSA2","EWWSC17VZPSA2"]
["Jahutusvõimsus","Nom","","kW","500","710","898","1,188","1,586","1,735"]
["Võimsuskontroll","Meetod","","","Muudetav","Muudetav","Muudetav","Muudetav","Muudetav","Muudetav"]
["","Minimaalne maht","","%","20","20","20","10","10","10"]
["Sisendvõimsus","Jahutus","Nom","kW","91.3","133.8","165.1","235.4","313.7","350.7"]
["EER","","","","5.48","5.31","5.44","5.05","5.05","4.95"]
["ESEER","","","","0","0","0","0","0","0"]
["Mõõtmed","Ühik","Sügavus","mm","3,750","3,822","3,822","4,508","4,750","4,874"]
["","","Kõrgus","mm","2,108","2,430","2,487","2,302","2,500","2,493"]
["","","Laius","mm","1,179","1,287","1,303","1,579","1,610","1,769"]
["Kaal","Ühik","","kg","3,247","4,082","4,346","6,310","7,530","8,250"]
["","Töökaal","","kg","3,375","4,349","4,660","6,900","8,300","9,200"]
["Vee soojusvaheti - aurusti","Tüüp","","","Sukelkest ja -toru","Sukelkest ja -toru","Sukelkest ja -toru","Sukelkest ja -toru","Sukelkest ja -toru","Sukelkest ja -toru"]
["","Vee maht","","l","96","168","199","320","380","480"]
["Vee soojusvaheti - kondensaator","Tüüp","","","Sukelkest ja toru","Sukelkest ja toru","Sukelkest ja toru","Sukelkest ja toru","Sukelkest ja toru","Sukelkest ja toru"]
["Kompressor","Tüüp","","","Inverterjuhitav ühe kruviga kompressor","Inverterjuhitav ühe kruviga kompressor","Inverterjuhitav ühe kruviga kompressor","Inverterjuhitav ühe kruviga kompressor","Inverterjuhitav ühe kruviga kompressor","Inverterjuhitav ühe kruviga kompressor"]
["","Kogus_","","","1","1","1","2","2","2"]
["Sound power level","Jahutus","Nom","dBA","99","105","105","106","107","109"]
["Mürarõhutase","Jahutus","Nom","dBA","80","86","86","87","88","89"]
["Jahutusaine","Tüüp","","","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A"]
["","Täide","","kg","130","180","180","190","320","350"]
["","Ahelad","Kogus","","1","1","1","2","2","2"]
["","GWP","","","631","631","631","631","631","631"]