{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Jahutusvõimsus","Nom","","kW","","","","6.80","6.80"]
["Ruumide jahutus","SEER","","","","","","6.43","6.43"]
["","Aastane energiatarbimine","","kWh/a","","","","371","371"]
["","Võimsus","Pdesign","kW","","","","6.80","6.80"]
["","Energiatõhususe klass","","","","","","A++","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Energiatõhususe klass","","","","","","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","","","","2,205","2,205"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","","","3.40","3.40"]
["","Aastane energiatarve","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Energiamärgistamise direktiiv","Jahutus","","","","","A"]
["","","Küte","","","","","A"]
["Küttevõimsus","Nom","","kW","","","","7.50"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Märkused","","","","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","","","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","(4) - Vt eraldi elektriandmete joonist"]