{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZQSG71L3V1B","FAA100BUV1B / RZQSG100L9V1B"]
["Jahutusvõimsus","Nom","","kW","6.80","9.50"]
["Ruumide jahutus","SEER","","","6.05","5.61"]
["","Aastane energiatarbimine","","kWh/a","394","593"]
["","Võimsus","Pdesign","kW","6.80","9.50"]
["","Energiatõhususe klass","","","A+","A+"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","6.33","6.81"]
["","SCOP/A","","","3.90","4.01"]
["","Energiatõhususe klass","","","A","A+"]
["","Aastane energiatarbimine","","kWh/a","2,123","2,378"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","3.21","3.01"]
["","Aastane energiatarve","","kWh","1,059","1,578"]
["","COP","","","3.61","3.41"]
["","Energiamärgistamise direktiiv","Jahutus","","A","B"]
["","","Küte","","A","B"]
["Küttevõimsus","Nom","","kW","7.50","10.80"]
["Märkused","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]