{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Korpus","Värvus","","","","Valge","Valge"]
["","Materjal","","","","Vaik","Vaik"]
["Mõõtmed","Ühik","","Kõrgus","mm","290","340"]
["","","","Laius","mm","1050","1200"]
["","","","Sügavus","mm","269","262"]
["Kaal","Ühik","","","kg","14","18"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","16.2","23"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","13.4","21.1"]
["","","","aeglane","m³/min","12.1","18.7"]
["","","Küte","kiire","m³/min","16.9","23"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","14.2","20.9"]
["","","Küte","aeglane","m³/min","12.7","18.7"]
["Helivõimsustase","Jahutamine","","","dBA","61","65"]
["","Soojendamine","","","dBA","61","65"]
["Mürarõhutase","Jahutus","","kiire","dBA","45","49"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","42","45"]
["Mürarõhutase","Jahutus","","aeglane","dBA","40","41"]
["","Küte","","kiire","dBA","45","49"]
["Helirõhu tase","Küte","","Keskmine","dBA","42","45"]
["Mürarõhutase","Küte","","aeglane","dBA","40","41"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","15.9","15.9"]
["","Tühjendus","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Standardsed lisatarvikud","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Märkused","","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Standardsed lisatarvikud","Screw cover","","","","","3"]