{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG100L9V1B"]
["Jahutusvõimsus","Nom","","kW","9.5"]
["Ruumide jahutus","SEER","","","6.11"]
["","Aastane energiatarbimine","","kWh/a","545"]
["","Võimsus","Pdesign","kW","9.50"]
["","Energiatõhususe klass","","","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","10.20"]
["","SCOP/A","","","4.01"]
["","Energiatõhususe klass","","","A+"]
["","Aastane energiatarbimine","","kWh/a","3,562"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,315"]
["","Energiatõhususe suhtarv","","","3.62"]
["","COP","","","3.61"]
["","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","A"]
["Küttevõimsus","Nom","","kW","10.8"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]