{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RXM35A5V1B9","FBA50A2VEB9 / RXM50A5V1B9"]
["Jahutusvõimsus","Nom","","kW","3.4","5"]
["Küttevõimsus","Nom","","kW","4","5.5"]
["Nimikasutegur","Energiatõhususe suhtarv","","","4.02","3.55"]
["","COP","","","4.02","3.83"]
["","Aastane energiatarve","","kWh","423","704"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","3.4","5"]
["","SEER","","","6.3","6.27"]
["","Aastane energiatarbimine","","kWh/a","189","279"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A+","A+"]
["","Võimsus","Pdesign","kW","2.9","4.4"]
["","SCOP/A","","","4.17","4.06"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.32","3.73"]
["","Aastane energiatarbimine","","kWh/a","973","1517"]
["Märkused","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(4) - Vt eraldi elektriandmete joonist"]