{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-F"]
[]
[]
[]
[]
["","","","","FBQ60C8VEB / RXS60F3V1B","FBQ60C8VEB / RXS60F4V1B"]
["Jahutusvõimsus","Nom","","kW","5.70 (3)","5.70"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","875","875"]
["","Energiatõhususe suhtarv","","","3.26","3.26"]
["","COP","","","3.41","3.41"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","B","B"]
["Küttevõimsus","Nom","","kW","7.00 (4)","7.00"]
["Märkused","","","","(1) - Energiamärgis: skaala vahemikus A (kõige efektiivsem) kuni G (vähem efektiivne)","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Aastane energiakulu: põhineb keskmisel aastasel kasutamisel 500 töötundi täiskoormusel (nimitingimustes)","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]
["","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m"]
["","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m; kõrguste vahe: 0 m"]
["","","","","(5) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]