{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B (Archived)"]
["Jahutusvõimsus","Nom","","kW","5.0 (2)"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","710"]
["","Energiatõhususe suhtarv","","","3.52 (1)"]
["","COP","","","3.83 (1)"]
["","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","A"]
["Küttevõimsus","Nom","","kW","5.50 (2)"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]
["Outdoor unit","","","","","RXS60L"]
["Jahutusvõimsus","Nom","","kW","","5.7"]
["Küttevõimsus","Nom","","kW","","7.00"]
["Nimikasutegur","Energiatõhususe suhtarv","","","","3.45"]
["","COP","","","","3.71"]
["","Aastane energiatarve","","kWh","","826"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","","A"]
["","","Küte","","","A"]
["Ruumide jahutus","Energiatõhususe klass","","","","A+"]
["","Võimsus","Pdesign","kW","","5.70"]
["","SEER","","","","5.86"]
["","Aastane energiatarbimine","","kWh/a","","340"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","A+"]
["","Võimsus","Pdesign","kW","","4.60"]
["","SCOP/A","","","","4.01"]
["","Aastane energiatarbimine","","kWh/a","","1606"]