{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MY1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7Y1B","FCAG125AVEB / AZAS125M7Y1B","FCAG140AVEB / AZAS140M7Y1B"]
["Jahutusvõimsus","Nom","","kW","","12.1 (1)","13.4 (1)"]
["Küttevõimsus","Nom","","kW","","13.5 (2)","15.5 (2)"]
["Ruumide jahutus","Võimsus","Pdesign","kW","","12.1","13.0"]
["","SEER","","","","5.40","6.00"]
["","Aastane energiatarbimine","","kWh/a","","1,345","1,300"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","","6.00","7.80"]
["","SCOP/A","","","","3.80","4.31"]
["","Aastane energiatarbimine","","kWh/a","","2,211","2,534"]
["Märkused","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Välisseade","","","","AZAS100M7Y1B"]
["Jahutusvõimsus","Nom","","kW","9.50 (1)"]
["Küttevõimsus","Nom","","kW","10.8 (2)"]
["Ruumide jahutus","Energiatõhususe klass","","","A+"]
["","Võimsus","Pdesign","kW","9.50"]
["","SEER","","","5.67"]
["","Aastane energiatarbimine","","kWh/a","586"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A"]
["","Võimsus","Pdesign","kW","6.00"]
["","SCOP/A","","","3.85"]
["","Aastane energiatarbimine","","kWh/a","2182"]
["Energiatõhususe klass","","","","A+++ ~ D"]