{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RXS35L3V1B"]
["Jahutusvõimsus","Nom","","kW","3.40"]
["Ruumide jahutus","SEER","","","6.35"]
["","Aastane energiatarbimine","","kWh/a","193"]
["","Võimsus","Pdesign","kW","3.50"]
["","Energiatõhususe klass","","","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","3.32"]
["","SCOP/A","","","4.90"]
["","Energiatõhususe klass","","","A++"]
["","Aastane energiatarbimine","","kWh/a","949"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","9.50"]
["","Tühjendus","OD","mm","VP25 (Välisdiam. 32, sisediam. 25)"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","3.74"]
["","Aastane energiatarve","","kWh","455"]
["","COP","","","3.50"]
["","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","B"]
["Küttevõimsus","Nom","","kW","4.20"]
["Märkused","","","","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist"]