{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZAG-A"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RZAG35A2V1B","FCAG50AVEB / RZAG35A2V1B","FCAG50AVEB / RZAG50A2V1B","FCAG60AVEB / RZAG50A2V1B","FCAG60AVEB / RZAG60A2V1B","FCAG71AVEB / RZAG60A2V1B"]
["Jahutusvõimsus","Min","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Max","","kW","4.5","4.5","6.0","6.0","6.5","6.5"]
["","Nom","","kW","3.5","3.5","5.0","5.0","6.0","6.0"]
["Ruumide jahutus","SEER","","","7.30","7.40","6.80","6.93","6.60","6.82"]
["","Aastane energiatarbimine","","kWh/a","168","166","257","252","318","308"]
["","Võimsus","Pdesign","kW","3.50","3.50","5.00","5.00","6.00","6.00"]
["","Energiatõhususe klass","","","A++","A++","A++","A++","A++","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","3.30","3.30","4.30","4.30","4.60","4.60"]
["","SCOP/A","","","4.30","4.41","4.30","4.35","4.25","4.39"]
["","Energiatõhususe klass","","","A+","A+","A+","A+","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","1,074","1,048","1,398","1,384","1,515","1,467"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","398","383","641","628","882","792"]
["","Energiatõhususe suhtarv","","","4.40","4.57","3.90","3.98","3.40","3.79"]
["","COP","","","4.30","4.41","3.71","3.75","3.40","3.53"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A","A","A","A","A"]
["","","Küte","","A","A","A","A","C","B"]
["Küttevõimsus","Nom","","kW","4.00","4.00","5.80","5.80","7.00","7.00"]
["","Min","","kW","1.40","1.40","1.50","1.50","1.60","1.60"]
["","Max","","kW","5.00","5.00","6.00","6.00","7.50","7.50"]