{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Jahutusvõimsus","Nom","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Küttevõimsus","Nom","","kW","","","","","","","","","","","","","","","","","","7.50","15.50"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","","","","","","","","","","","","","3.30","3.30","3.30","3.39","3.39","2.50"]
["","COP","","","","","","","","","","","","","","","","","","","","3.97","3.61"]
["","Aastane energiatarve","","kWh","","","","","","","","","","","","","","","","","","1,003"]
["","Energiamärgistamise direktiiv","Jahutus","","","","","","","","","","","","","","","","","","","A"]
["","","Küte","","","","","","","","","","","","","","","","","","","A"]
["Ruumide jahutus","Energiatõhususe klass","","","","","","","","","","","","","","","","A","A","A","A++","A++"]
["","Võimsus","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10","5.10","6.80","6.72","6.44"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","","","","","","","","467","467","467","350","355","1,249"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","","","","","","","","","","","","","A","A","A","A+","A+"]
["","Võimsus","Pdesign","kW","","","","","","","","","","","","","","6.00","6.00","6.00","6.33","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80","3.80","4.20","4.20","4.27"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","","","","","","","","2,211","2,211","2,211","2,110","2,110","3,795"]
["Märkused","","","","","","","","","","","","","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","","","","","","","","","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","","","","","","","","","","","","","","","(3) - Vt töövahemiku kohta eraldi joonist","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","","","","","","","","","","","","(4) - Vt eraldi elektriandmete joonist","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]